1. Description:
   This driver is supporting for QNX6.2.1 for X86 and ARM CPU.
It is for Serial port only.

2. Content
   devi-urtc.tar     --   a. for X86
                          b. have been test

   devi-urtc-arm.tar  --  a. for ARM
                          b. test yet.

3. Setup (example for X86)
   a. copy devi-urtc.tar into your directory in your computer
      #cp /fs/floppy/devi-urtc.tar  /your directory

   b. decompress devi-urtc.tar
      #tar xvf devi-urtc.tar
   c. copy devi-urtc into /usr/photon
      #cp ./devi-urtc /usr/photon
   d. run the driver
      # devi-urtc urtc fd -d/dev/ser1 abs
      *Note: /dev/ser1 is COM1
             /dev/ser2 is COM2
             user should know where your device is.

4. Calibration
   a. QNX has supported calibration tool called "calib", so
      usr just run the "calib".
      #calib