POSTouch driver v1.3C Copyright (c) 2003-2009
Release date: 04-15-2005

Description:
------------
INSTALL.BAT - Insatllation program
-This batch file copy all files related to DOS touch to the driver you specify.
-Usage: INSTALL SourceDIR  DestinationDIR , SourceDIR=Source disk or directory name.

idTouch.com  - Driver for POSTouch Controller
-This program are mouse drivers for POSTouch Touch Controller, which support
 many touch protocols(POSTouch, EloTouch, MicroTouch protocols).
 Help can be obtainded with the '/?' command line option.
-Basically it were written to use as small amount of memory as possible.
 They try to install themselves into upper memory first if availbale, so do
 not load high them with external utilities (like DOS lh command).
-Usage: 1.idTouch     .... Load driver on standard COM1 port(0x3F8, IRQ=4)
        2.idTouch /2  .... Load driver on standard COM2 port(0x2F8, IRQ=3)
        3.idTouch /5 /I9 /AD400 .... Load driver on COM5 with Adress=0xD400, IRQ=9
        4.idTouch /U  .... Unload driver
        5.idTouch /?  .... Get help message
        where :
		/n    - where n is the COM port number from 1 to 6(Default=1)
		/In   - Force IRQ number (n is in hex: n=3-F)
		/Axxx - Force COM port I/O address
		/B    - Force Button Mode
		/S    - Force Stream Mode
		/Mn   - Force Emulation Mode (n is in dec: n=0-3)
		/U    - Release driver
		/?    - Show help

idTouch.vpr  - Video mode parameters of your Video Card
-This file will be loaded with idTouch.com to support various video mode of
 your video card. Use UTC.exe to edit this file if your application do change
 video mode and mouse can not map to correct touch position within the AP.

GetVMode.com- Get video mode history that the last application been enter
-The touch driver trap int10 entry and log the video mode that the application
 try to enter. This program is useful for the application that enter a video
 mode with resolution not support by the default driver setting.
-This program must be revised if idTouch.com have modified.
-Usage: GetVMode

UTC.exe      - Setup utility for POSTouch controller.
- This utility let you change working parameters of POSTouch controller.
-Usage: 1.UTC ....... Invoke the utility with selectable menu functions.
        2.UTC /Cn ... n=3,5 or 9, Invoke 3/5/9 points calibration routine directly.
                      (After calibration procedure, the utility will jump to freedraw routine!!
                       Press 'ESC' key once will clean screen; twice to leave freedraw and end program.)

CAL3P.exe    - VESA display mode calibration utility for POSTouch controller.
- This utility let you calibration the POSTouch controller on each VESA display mode.

B55.BAT     - Auto setting the POSTouch driver on B55 motherboard.

B77.BAT     - Auto setting the POSTouch driver on B77 motherboard.

NM9835.BAT  - Auto setting the POSTouch driver that use the NetMos Nm9835 PCI serial port.

F81216D.BAT - Auto setting the POSTouch driver that use the Fintek F81216D serial port.                       

LoadUTC.bat - Scan COM port & install driver.
-This program assume your COM port use standard I/O port & IRQ
-Usage: LoadUTC
