Application note for install POSTouch driver on NetMos PCI serial port under Linux

Cause of the NetMos PCI serial port cannot be auto install by Linux,
 please follow the below step to install the POSTouch on NetMos PCI serial port.

1. Please install the NetMos serial auto install procedure.
   It will auto setting the Serial Port on ttyS4 and ttyS5 when Linux booting.
   
   Install procedure:
   
   Get NetMos driver in .Common\Netmos\Linux\v1.0
   
     Install NetMos Driver
       1.Unpack tar.gz package file :
        #tar -zvxf  v1.0.tar.gz

       2.'cd' to package directory :
        #cd v1.0

       3.Execute the setup.serial script :
        #./setup.serial
   
2. Install the POSTouch driver
   Install procedure please reference the ReadMe.txt file.
