Content:
	QNX		-- QNX driver.

	Fedora		-- Fedora Core 1 and Fedora Core 2 xfree driver and USB character driver.

	Mandrake\9.0	-- Mandrake9.0 xfree driver and USB character driver.
	Mandrake\10.0	-- Mandrake10.0 xfree driver and USB character driver.
			How to install:
			 1. See the ReadMe_serial to install RS232 touch panel driver.
			 2. See the ReadMe_USB to install USB touch panel driver.
			     touch.o.gz is USB device character driver.
			 3. RS232 and USB common to use xfdrvtouch_drv.o as xfree driver
			touch.calib is 3 points data.
			Release distribution is GTK1.0. Please, check your task panel into autohide mode for full screen.

	RedHat9.0	-- RedHat9.0 xfree driver and USB character driver.
			How to install:
                         1. See the ReadMe_serial to install RS232 touch panel driver.
                         2. See the ReadMe_USB to install USB touch panel driver.
                             touch.o is USB device character driver.
                         3. RS232 and USB commonly to use xfdrvtouch_drv.o as xfree driver
			touch.calib is 3 points data.
			Release distribution is GTK2.0.

	RedHat8.0	-- RedHat8.0 xfree driver.
			How to install:
			 1. See the ReadMe_serial to install RS232 touch panel driver.
			 2. RS232 use xfdrvtouch_drv.o as xfree driver
			touch.calib is 3 points data.
			Release distribution is GTK1.0. Please, check your task panel into autohide mode for full screen.

	Calib_3P232_GTK1.0.tar.gz	-- RS232 touch panel 3 points calibration utility with GTK>=1.0 && <=2.0.
	Calib_3P232_GTK2.0.tar.gz	-- RS232 touch panel 3 points calibration utility with GTK2.0 later.
	Calib_3PUSB_GTK1.0.tar.gz	-- USBtouch panel 3 points calibration utility with GTK>=1.0 && <=2.0.
	Calib_3PUSB_GTK2.0.tar.gz	-- USBtouch panel 3 points calibration utility with GTK2.0 later.
	FreeDraw_GTK1.0.tar.gz		-- Free Draw Utility with GTK>=1.0 && <= 2.0.
	FreeDraw_GTK2.0.tar.gz		-- Free Draw Utility with GTK2.0 later.
	Linear232_GTK1.0.tar.gz		-- RS232 touch panel linear utility with GTK>=1.0 && <=2.0.
	Linear232_GTK2.0.tar.gz		-- RS232 touch panel linear utility with GTK2.0 later.
	LinearUSB_GTK1.0.tar.gz		-- USB touch panel linear utility with GTK>=1.0 && <=2.0.
	LinearUSB_GTK2.0.tar.gz		-- USB touch panel linear utility with GTK2.0 later.

Note:
   *** If your linux runs with GTK2.0, please install XXXX_GTK2.0.tar.gz package.
   *** GTK2.0 supports full screen feature, but GTK1.0 not.

   We recommend you upgrade your GTK package to 2.0 later. And you can use GTK2.0 Utility.

   *** If you install XXXX_GTK1.0.tar.gz package, you need to AutoHide X windows taskbar by Manually 
	to make the utility to occupy all screen area. If you don't, the mouse data will be wrong.
