## Properties

- A Properties page will be created for each touchscreen controller installed by EloSetup and for each serial port reserved for a controller, even if that controller is not present. A number will be assigned to each Properties page that is related to the order in which controllers or ports were detected or enumerated. Each Properties page contains information extracted from the touchscreen controller and the system about the monitor, touchscreen, controller, and internal driver.

### Screen Information

> #### Properties 1

> ####

> #### Windows Monitor Number

> - Windows monitor number lists the monitor that corresponds to the "Windows Monitor" from the Windows Display Properties control panel.

> #### Touchscreen Type

> - Touchscreen Type lists the Elo touchscreen used by its marketing name, i.e., AccuTouch for Elo's five-wire resistive touchscreen

> #### Installed On

> - Installed On indicates USB or lists the Windows COM port that a serial touchscreen is installed on.

> #### Controller Model

> - Controller Model lists the marketing model number of the controller attached. It also lists the revision of the firmware loaded in the controller.

> #### Controller Status

> - Controller Status indicates either "Working properly" or reflects any errors reported from the controller.

> #### Driver Version

> - Driver Version lists the version number of the internal driver being used for serial and USB devices as appropriate.

Each Properties page also contains a Screen information section that has two functions:

- The Identify Monitor button will display the Elo logo on the monitor associated with this Properties page for about one second each time this button is touched.

- The EloVA icon will launch the video alignment program only for the monitor associated with the current Properties page. Running EloVA from the Properties page avoids the need to align all monitors in a multiple monitor application when only a single monitor alignment is desired.

> If a serial port is reserved for a touchscreen controller that is not actually installed, the only information contained in the Screen information section of the associated Properties page will be the number of the Windows COM port. No Screen configuration icons will be displayed.

> Each Properties page also contains an Advanced section.

> Advanced page contains an Option and Right click on hold section. Option section has:

- Show right mouse button tool launches this feature for this monitor. See Right Mouse Button for a complete description of this feature.
- Disable Touch stops touch information from reaching Windows for this touchscreen. This feature may also be activated from the Tool Tray utility. Disabling touch has no effect on the operation of the standard mouse.

> ### Right Click on Hold

> Right Click on Hold is a new feature added in version 4.20. This feature allows new and efficient way of creating right clicks on the touch screen without needing to run the Right Mouse Button Tool. If the user touches the screen and continues to touch, a right click is generated on the screen, if the users remains within the Right click area and after the Right click delay time-out has occured. The right click delay allows the users to perform other touchscreen operations normally.When the user touches the screen and holds his finger down, an animated clock is painted at the location, the animated clock continues to tick and generates a right click at the location after it completes.

> - Enable right click on hold: If checked, it enables this feature for this screen, otherwise, it is disabled.

> - Apply to all touchscreens: If checked, the current values are set to all touchscreens when "Apply" or "Ok" button is clicked.

> - Right click delay: Defines the right click delay value in milliseconds. The right click delay allows the users to perform other touchscreen operations normally.
> - Right Click Area: Touching within this area generates a right click. This area allows the user the flexibility to touch within a larger area.

> NOTE:

> o Right click on hold feature is enabled only in "Mouse emulation" touch mode.

> o When Right click on hold feature is turned on, Drag Delay value is set to a minimum of 25 milliseconds.

#### Properties 2 Tab

> ####